<ep> f30  <id #keyboard> 
<VideoMode desktop> <t 4000> <eop>
0 <ln -1> "Display Test Mode 2" ,
<ln 1> "When DMDX is waiting for a request and there is no active display it displays", 
<ln 2> "a test screen with information about the millisecond callback latencies",
   <ln 4> "timelimit 4000";
5  "Test Mode 2" / <testmode 2>;
+3  <cr> "fwdmask" %10/ * "target" %2 / "make a response" ;
+3  <cr> "fwdmask" %10/ * "target" %2 / "make a response" ;
+3  <cr> "fwdmask" %10/ * "target" %2 / "make a response" ;
0 <cr 0>"done";
0“end” l;