<ep> f30  <id #keyboard>
<VideoMode desktop> <eop>
0 <ln -1> “Display Test Modes 5 and 3” ,
<ln 1> "When DMDX is waiting for a request and there is no active display it displays", 
<ln 2> "a test screen with information about the millisecond callback latencies",
 <ln 3> "but it only monitors millisecond callback latencies while DMDX is waiting for an input";
5 <nfb 0> <ntl 0>  “Test Mode 5 (only monitors during input)” / <testmode 5>;
+1 "fwdmask" %10 / * "target" %2 / "make a response";
+2 "fwdmask" %10 / * "target" %2 / "make a response";
0 “Test Mode 3 (only monitors during display)” / <testmode 3>;
+3 "fwdmask" %10 / * "target" %2 / "make a response";
+4 "fwdmask" %10 / * "target" %2 / "make a response";

+1 <nfb> <ntl> c "Repeat it?" * <bic -5>; 
0 “end” l;