<ep> <!t 148500> <id mouse> <cr> <mr +button 1> <azk> f10 <id "keyboard"> 
<vm desktop> <!testmode 3> <dbc 0> <dwc 255000>
<id recordvocal 150,777> <id digitalvox 77> </ep>
0 "This itemfile is for RecordVocal/DigitalVox testing." @-2 ,
   "WAV output must be looped to Input" @-1,
   "(so the TimeDX Sound Latency test works)",
   "use the Stereo Mix device if available" @1,
   "RTs should be in the 1000ms range" @2,
   "First a couple of items to get rid of startup variability" @4;

+1 "first" / <wav 2> "1sec50ms" %0 <svp start> / * <%ms 1000 emit> / "beep" ;
+2 "second" / <wav 2> "1sec50ms" %0 <svp start> / * <%ms 1000> /  "beep" ;

0  “And now a little Test Mode 9 action” , @1 "this should gather 100 ~1000 ms RTs"
	<testmode 9> <set c1=100>;
+3   "%d to go" <sprintf 1> / <wav 2> "1sec50ms" %0 <svp start> / * <%ms 1000> /  
	"beep" <dec 1> <bicgt 1,0,-3>;

0 "done";
0 L "The End" ;